DISCUSS
Required equipment for night flight

L(IE) CAR

All Instrument and circuit breaker panel Lights
All Exterior Lights

Operable Communication radio

Attitude gyro

Radar altimeter

Helicopter preparation for night operations

Preflight should be conducted during daylight when possible.  If not, a white lens flashlight should be used.  Red lens will not detect oil and hydraulic leaks.

In addition to normal preflight, pilot must ensure:

external and internal lighting systems are working

rad. alt

stby bat voltage and right seat att ind.

all windows clean

check NOTAMS for limitations on night ops at field

perform Instrument Checklist while taxiing for takeoff
Night autorotations

Shall only be practiced from the 90 ° or straight in positions.

Searchlight shall be turned on by 200’ AGL

Shall only be practiced on a lighted runway with a crash crew on duty.

Shall be power recovery no lower than 10’
INTRODUCE

Partial panel climbs and descents

Full panel unusual attitudes

1. LEVEL THE WINGS

2. LEVEL THE NOSE

3. CENTER THE BALL

4. SET POWER FOR 80KIAS.  STOP ANY CLIMB OR DESCENT, ACHIEVE 80

5. RECHECK WINGS NOSE AND BALL

6. EXECUTE STANDARD RATE CLIMB OR DESCENT TO BASE ALTITUDE

7. EXECUTE LEVEL STANDARD RATE TURN TO BASE HEADING

PRACTICE

COMM/NAV checklist
ITO checklist

ITO

Standard Instrument Departure
Leveloff checklist
Level speed change

Level standard rate turns to headings

Turn pattern

Vertical S-1 pattern

OSCAR pattern

Magnetic compass turns

Partial panel straight and level flight

Partial panel turns

TACAN/VOR-DME approach

Instrument autorotation
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