Basic Transitions

Cruise to Climb


Power to Max allowable


Attitude exhaust stacks on horizon


Trim  RIGHT and UP


@ 120 kts, lower nose to hold speed


Trim

Climb to Cruise


200 ft prior, lower nose TOWARDS level


Trim  LEFT and DOWN


Approaching Cruise Speed Power to 600-650 or 750-800 ftlbs


Attitude Level Flight


Trim  LEFT

Cruise to Descent


Power to 300 ftlbs


Attitude nose down to maintain Cruise Speed


Trim  LEFT and UP

Descent to Cruise


100 ft prior, Power to 600-650 or 750-800 ftlbs


Attitude raise to level flight


Trim  RIGHT and DOWN

Level Speed Changes

Power to 300

When below 150 Gear Down

Approaching 100 kts, power to 500-550 to maintain 100 kts

When on speed, heading, and alt, LANDING CHECKLIST up to FLAPS

Perform Turns as IP says

Power to 100

When below 120 Flaps Down

Approaching 90 kts, power to 600 to maintain 90 kts

Check full flaps and report Gear Down Flaps Down Landing Checklist Complete
Perform Turns as IP says

Power to MAX

Check below 120 Gear UP Flaps UP Landing Lights Off

Approaching 170 kts, power to 750-800.

Cloud Clearances

Class C Airspace:
3 SM Vis, 500 Below, 1000 Above, 2000 Horizontal

Class E below 10k:
3 SM Vis, 500 Below, 1000 Above, 2000 Horizontal

Class E above 10k:
5 SM Vis, 1000 Below, 1000 Above, 1 SM Horizontal

Illness, Medication, Stress, Alcohol, Fatigue, Eating
