Ditching

Speed, Clean,Check, FTHR, Look (DIR), Lock, Airstart, Bail, FuelOff, T handle, Flaps, Canopy, Exit, LPU

OPTIONAL:
Mayday/7700, Parachute unfasten, O2 mask off, Battery Off.



Ditch into the wind if calm, parallel to swells if moderate, upwind of swell on high.

Airborne Damaged Aircraft

Maintain control of aircraft, if not controllable 
BAIL OUT
Climb





AS REQUIRED

Check flight characteristics above 5,000 feet AGL in the landing config, decreasing at 10kts to land speed.

Fly a wide or straight-in approach and land as soon as possible
OCF Recovery Procedures

Controls

POSITIVELY NEUTRALIZE
PCL

IDLE

Altitude

CHECK


If recovery from OCF cannot be accomplished by 5,000ft AGL, bail out

AOA, airspeed, turn needle
CHECK


Application of spin recovery controls when not in spin may aggravate the OCF condition

Gear/flaps


UP

Rudder



FULL OPPOSITE TURN NEEDLE

Stick



FORWARD OF NEUTRAL(erect)/NEUTRAL(inverted)

Controls



NEUTRALIZE WHEN ROTATION STOPS

Recover from unusual attitude
4390 Preparation

Securing Rear Cockpit

Seat



LOWER TO FULL DOWN

Harness, parachute, O2 equip
SECURE

Fasten Leg Straps Through helmet bag handles
Fasten Chest Strap

Wrap Hose Cord and Clip

Fasten Lap Buckle

Run through housing and fasten

Lock reel and tighten harness

Complete solo checklist

Cockpit lights


OFF

Switches


BATTERY ON, INV #2 ON, ALL OTHERS AS REQUIRED

Inspect for and secure loose equipment

Aft canopy


CLOSE/LOCK
JACKET REVIEW

SFS TEST COMPLETE

ATS

SPIN

UA RECOVERY

HAPL

LAPL

PPEL

LAPL(P)

PPEL(P)
