Any EP

One-half Cuban Eight

First 210deg of a loop, a half roll to upright position, and a 45deg diving pull out.

Config:
Aerobatic cruise.
Checklist
Clearing turn


During last 90 of turn, lower nose to accel to 200 KIAS.  Roll out on a section line at 200 KIAS


Check wings level and clear airspace above you.  Check and report entry altitude.


Commence AGSM and start a smooth pull-up to 3.5Gs


Recheck wings level as you pass horizon.  Tilt head back to locate opposite horizon.


Allow the nose to fall through the horizon to 30deg below and slow nose movement.


Commence a roll in either direction, using aileron and rudder and slight down press to 45degdown


Commence a smooth pullout to straight and level balanced flight.
Split-S
Rapidly changing direction of flight using potential energy of altitude.  1500 feet usually lost

Config:
Aerobatic cruise.
Checklist
Clearing turn

Procedure:


Reduce power to idle and maintain altitude while slowing to 130 KIAS.


Raise the nose to place exhaust stacks on horizon, relax backstick pressure and roll in either dir.


Once inverted neutralize ailerons and apply slight forward stick to maintain straight and level.


Verify wings level, and apply back stick pressure pulling nose through the horizon.


Check oil pressure within normal limits.  Reset aerobatic cruise power and report oil pressure.
Immelman
Quick means of changing direction of flight using airspeed to trade for altitude.

Config:
Aerobatic cruise.
Checklist
Clearing turn

Procedure:


During last 90 of turn, lower nose to accel to 200 KIAS. Roll out on a section line at 200 KIAS


Check wings level and clear airspace above you.  Check and report entry altitude.


Commence AGSM and start a smooth pull-up to 3.5Gs


Recheck wings level as nose passes horizon.  Tilt head back to locate opposite horizon.


As nose approaches a point 20deg above opposite horizon, neutralize back stick pressure.


Roll in either direction to upright. Finished when level flight on recip heading.  100 KIAS.
