BAC Maneuver
Transition to BAC (Power to 450, Gear down, Power back to 650, hold 120, perform Landing Checklist)
Execute a missed approach (1015, nose to 6-8, Gear up, 3 up and locked, @120 do a 45 deg AOB turn, 


climb 1000 feet, 200 feet prior, level off and transition to 150 knots.

Approach Maneuver

Roll into a right SRT (2 needle widths) for 90deg of heading change.
After completion of turn, note time and fly outbound for 3 minutes.

Power to 300 slow to 120

@ 120, lower nose to 2deg down and descend for 1000 feet at 120 knots

25 feet prior to level off, power to 450 and raise nose to slow cruise (1½ deg nose up)

At the end of three minutes, commence a left SRT for 210deg
Roll wings level after 210 deg

Go to BAC by lowering gear, nose to 2-4 deg down.

Descend 120 knots for 500 feet.

During descent report landing checklist

100 feet prior to end of 500 feet descent, transition to level flight. (power to 700, nose 2deg up)

Maintain this level flight for 1 minute.

At end of minute, execute missed approach (1015, 6-8 nose up, gear up, landing lights off)


@120 knots of climb start right SRT for 45deg of heading change, roll out


Climb back to original altitude (1500 feet)


200 feet prior to level off commence transition to normal cruise.

EPs

Electrical fire (IMC)


Electrical/Unknown Origin Fire (IMC)



Attempt to locate/isolate source of fire/fumes




If unsuccessful continue:



Utility bus switches
OFF



All other nonessentials
OFF



Airspeed

REDUCE (as required)



100 % Oxygen 

DON (as required)



Cockpit environmental control/aft cockpit outside air
OFF




If fire persists:



Bail out (altitude permitting).




If fire extinguishes:



Land as soon as possible.
Smoke or fume elimination


Smoke of fume elimination



100 % Oxygen

DON



Airspeed

REDUCE



Cockpit environmental control/aft cockpit outside air
FRESH AIR INCREASE/ON




If smoke or fumes remain, obstructing sight for landing, or head buildup


Canopy


EMERGENCY OPEN
