Partial Panel
Execute the EP for inverter failure.
Go to straight and level partial panel scan.

“I have a gyro failure; emergency procedures completed with negative results; on partial panel scan.”
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Partial Panel Straight and Level
Partial Panel Timed Turns
For heading changes of 30deg or more, use 1 needle width, for 2/3 * deg turns for time
For heading changes of 29deg or less, use 2/3 needle width, 1 * deg turns for time

Partial Panel Enroute Descent

500 ftlbs, constant A/S, wings level
back to 650 ftlbs when 100 feet above level off alt.

EPs

Engine fire in flight

Engine fire in flight:


Fire

CONFIRM


Engine shutdown
EXECUTE



Cockpit air
OFF




If fire persists:



Bail Out

EXECUTE




If fire extinguishes:



Engine Failure
EXECUTE




If no fire indications:



PEL

EXECUTE
Chip light

Chip light:


PEL

EXECUTE (850ftlbs)



If engine failure/malfunction occurs:



Engine shutdown
EXECUTE



Engine Failure
EXECUTE
