Partial Panel Unusual Attitudes
Hold stick pressure as you recognize whether nose high or nose low by the actions of A/S and T/N
If A/S is approaching 200, power to idle.

Using smooth coordinated rudder and aileron, center the ball, and level the wings with T/N

Smoothly and slowly relax stick pressure as necessary to stop A/S

When A/S is stopped, adjust nose position until the VSI stabilizes at 0.

Reset power to normal cruise if needed.

EPs

Inverter Failure

Inverter Failure:


Other inverter

SELECT



If annunciator remains illuminated:



Electrical Command
TAKE



115-VAC, 1-amp CB
IN



Inverter Control relay CB
IN

Generator Failure
Generator Failure:


Starter Switch

OFF (both cockpits)


Generator Switch

ON (reset)




If annunciator remains illuminated:



Electrical command 
TAKE



Generator Switch

ON (reset)




If generator does not return to line:



Electrical Load

REDUCE



Land as soon as practicable
Gyro Failure


Gyro Failure:

Partial Panel


Partial Panel:

Limited Use of Magnetic compass


Limited Use of Mag Compass:
