I-2203
CD: 274.7  Ground: 251.15
Tower: 306.925   Dep: 278.8
· ATIS: “Info___, 1,500 OVC, vis 3 miles in light rain, altimeter 29.98, duty RW is 5”
· Complete the first 11 steps of instrument checklist

· **Switch to CD*** “North Whiting Clearance Delivery, N6E, IFR to Bob Sikes, clearance on request”
· “Clearance Delivery, N6E, ready to copy”
· “N6E, is cleared to the Bob Sikes Airport via the Crestview One departure to Crestview. Maintain 7,000. Departure Freq will be 278.8, squawk______”
· “North Whiting Ground Control, N6E taxi with information___”
· “N6E, taxi to runway____”
· Finish Checklist

· Ensure radios, NAVIDS, transponder and CDI set for departure. VOR audio switch to on.
· “North Whiting Tower, N6E, take-off”
· “North Whiting Tower, N6E, after take-off, turn left to 010, switching to Departure, cleared for take-off”
· “Pensacola Departure, N6E, off North Whiting, passing 800 for 7,000”
· “N6E,  Report level 7000”
· “N6E, Wilco” IGP
· “Pensacola Departure, N6E, level 7,000”
· “N6E, contact Crestview approach on 307.375 when inbound to CEW 
· “N6E, approach on 307.375 when Inbound” IGP
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· “Crestview Approach, N6E, estimating Crestview at time + 6=  ___, 6000 with negative info” IGP 

· ATIS: Weather at Bob Sikes is 900’ OVC, 1 mile vis in light rain, altimeter ___, RW ___
· “Roger Weather and Runway, altimeter _______”

Practice:

Radial Intercepts: 263 radial to  ___ radial.
Track inbound to Crestview. IGP
Station passage using CEW
VOR Holding:

· “N6E, is cleared to hold East of the Crestview VORTAC on the 090 radial, expect further clearance at _______”
· Emphasize 6T’s, holding entry report (PTA), entry orbit (teardrop), now wind orbit, correction orbits)

· “N6E, is cleared to hold East of the Crestview VORTAC on the 090 radial, expect further clearance at time _____” IGP
· “Crestview Approach, N6E, holding at Crestview, _____, 7000” IGP
· “Crestview Approach, N6E, request confirmation on EFC”

· “N6E, roger, EFC time _______”
Shuttle Descent: Clear for decent to 4,500. At expiration of the EFC, clear for the CEW VOR C approach. (Fail DME, radio and Nav #3)

· “N6E, you are cleared to descend to 4500”
· “Crestview Approach, N6E, leaving 7000 for 4500” IGP
· “Crestview Approach, N6E, departing holding”

· ATIS: Weather at Bob Sikes is 900’ OVC, 1 mile visibility in light rain, altimeter _____, RW ___
·  “Crestview Approach, N6E, roger your weather and runway, altimeter _____, request VOR-C Approach”
· “N6E, roger you are cleared for the VOR C approach”

· “Crestview Approach, N6E, cleared for the VOR-C approach, report VOR outbound” IGP
· “Crestview Approach, N6E, departing holding”

Procedure Turn: 6T’s, appropriate voice reports, proper procedure for intercepting FAC is used.

· “Crestview Approach, N6E, VOR outboud” IGP
· BAC, LCL, Talk: “Bob Sikes Tower, procedure turn inbound, gear down and locked”
· Analyze MAP: “Bob Sikes Tower, N6E, VOR inbound”
· “Bob Sikes Tower, N6E, missed approach, runway not insight”
· “Crestview Departure, N6E, request my alternate, Navy North Whiting, via Direct, alt 7000, 2+05 fuel remaining, 0+10 time enroute” IGP
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