· ATIS: “Info___, 2000 SCT, vis 5 miles in haze, altimeter 30.02, duty RW is 5”
· Complete the first 11 steps of instrument checklist

· **Switch to CD*** “North Whiting Clearance Delivery, N6E, IFR to Monroe County Airport, clearance on request”
· “N6E, is cleared to the Monroe County Airport via the BAEYE ONE Departure to BAEYE, V-3 to Monroeville. Maintain 6,000. Departure Freq will be 278.8, squawk______”
· “North Whiting Ground Control, N6E taxi with information___”
· “N6E, taxi to runway____”
· “N6E, roger”
· Finish Checklist.  TWIST AND TOGGLE

· Ensure radios, NAVIDS, transponder and CDI set for departure. VOR audio switch to on.
· “North Whiting Tower, N6E, take-off”
· “North Whiting Tower, N6E, after take-off, turn left to 010, switching to Departure, cleared for take-off”
· “Pensacola Departure Control, N6E, off North Whiting, passing 800 for 6,000”
· “N6E,  Report level 6000”
· “N6E, Wilco” IGP
· “Pensacola Departure, N6E, level 6,000”
· “N6E, contact Jacksonville Center on 251.1” 
· “N6E, contacting Jacksonville center on 251.1” IGP
· “Jacksonville Center, N6E, estimating PENSI at _____, level 6000”

At PENSI, single NAVAID Primary CEW 115.9, secondary NUN 108.8
· “Jacksonville Center, N6E, PENSI, over”
· “Jacksonville Center, N6E, PENSI _____, 6000, estimating BAEYE at time +5=          , ATMOR” IGP
At BAEYE, dual NAVID, primary CEW 115.9, secondary MVC 115X, Monroeville becomes primary after turn.
· “Jacksonville Center, N6E, BAEYE, over”

· “Jacksonville Center, N6E, BAEYE time, 6000, estimating ATMOR at time + 6=          , Monroeville” IGP
ATMOR, TACAN only, primary MVC 115X
· “Jacksonville Center, N6E, ATMOR, over”

· “Jacksonville Center, N6E, ATMOR time, 6000, estimating Monroeville at time + 11=         , destination” IGP
· “N6E, contact Monroeville Approach Control on 351.9, with negative information.”

· “N6E, contacting approach on 351.9”
· “Monroeville Approach, N6E, estimating Monroeville at time + 11-= _____, 6000, with negative information.”
· “N6E, cleared to hold ____ of the Monroeville VORTAC on the _____radial, left turns, expect further clearance at _____. Expect radar vectors to final for the Monroeville VOR A approach”

· “Monroeville Approach, N6E, cleared to hold ____ of the Monroeville VORTAC on the _____radial, left turns, expect further clearance at _____. Expect radar vectors to final for the Monroeville VOR A approach” IGP
· “Monroeville Approach, N6E, holding at Monroeville, time, 6000”
· “Monroeville Approach, N6E request confirmation on EFC”
· “N6E, roger, Expected Further Clearance  time _______”
Shuttle Descent: Clear for decent to 3400. At expiration of the EFC offer radar vectors for the MVC VOR A Approach
· “N6E, you are cleared to descend to 3400”
· “Monroeville Approach, N6E, leaving 6000 for 3400” IGP
· “Crestview Approach, N6E, departing holding”

· “N6E, Ident”
· “N6E, Monroeville Approach, radar contact ___ miles ____ of Monroeville. Turn L/R heading ____. These will be radar vectors to the final approach course for the VOR A approach to Monroe County Airport. Monroeville weather is Weather at Monroe County _____ OVC, __ mile visibility in light rain, altimeter ______, circle to land runway 21, over”
· “Monroeville approach, N6E, turn L/R heading ​​​____, roger the weather and runway, altimeter ______” 

· “N6E, now ___ miles from MVC VOR, turn L/R heading ___, intercept the final approach course at or above 3400, cleared for the VOR A approach to Monroe county Airport, circle to land 21. Contact Monroe County Tower this freq when established inbound on the final approach course, out”
· “Monroeville approach, N6E, cleared for the approach, contact Monroe County Tower this frequency established inbound on the final approach course, out”

· BAC, LCL, Talk, MA

· ”Monroe County Tower, N6E, final approach course inbound, gear down and locked”
· “Monroe County Tower, N6E, circle north, cleared to land RW 21”
· “Monroe County Tower, N6E, missed approach, runway not insight”

· “Monroeville Departure, N6E, request my alternate, Navy North Whiting, via direct, alt 6000, 2+?? Fuel remaining, 0 + 18 time enroute” IGP
