· ATIS: “Info___, 800 OVC, vis 4 miles in light fog, altimeter 30.00, duty RW is 32”
· Complete the first 11 steps of instrument checklist

· **Switch to CD*** “North Whiting Clearance Delivery, N6E, IFR to Monroe County Airport, clearance on request”
· “Clearance Delivery, N6E, ready to copy”
· “N6E, is cleared to the Monroe County Airport via the BAEYE ONE Departure to BAEYE, V-3 to Monroeville. Maintain 8,000. Departure Freq will be 278.8, squawk______”
· “North Whiting Ground Control, N6E taxi with information___”
· “N6E, taxi to runway____”
· “N6E, roger”
· FINISH CHECKLIST, TWIST AND TOGGLE

· Ensure radios, NAVIDS, transponder and CDI set for departure. VOR audio switch to on.
· “North Whiting Tower, N6E, take-off”
· “North Whiting Tower, N6E, after take-off, turn right to 340, switching to Departure, cleared for take-off”
· “Pensacola Departure Control, N6E, off North Whiting, passing 800 for 8,000”
· “N6E, ident”
· “N6E, Pensacola Departure Control, radar contact __ miles Northwest of North Whiting, report level at 8,000”

· “N6E, Wilco” IGP
· “Pensacola Departure, N6E, level 8,000”
· “N6E, contact Jacksonville Center on 251.1” 
· “N6E, contacting Jacksonville center on 251.1” IGP
· Identify PENSI using Crewtview TACAN radial and DME

· “Jacksonville Center, N6E, PENSI”

· “Jacksonville Center, N6E, BAEYE”
· “Jacksonville Center, N6E, ATMOR”
· “N6E, contact Monroeville Approach Control on 351.9”

· “N6E, contacting approach on 351.9”
· “Monroeville Approach, N6E, ATMOR, with negative information”
· “N6E, Weather at Monroe County is _____ OVC, __ mile visibility in light rain, altimeter ______, duty runway is _____, Expect the Monroeville VOR C approach”
· “Monroeville Approach, N6E, roger your weather and duty runway, altimeter is ________.  Expect the Monroeville VOR C approach” IGP
Terminal Descent: Clear for decent to 4500. 
“N6E, you are cleared to descend to 4500”
· “Monroeville Approach, N6E, leaving 8000 for 4500” IGP
· “N6E, you are cleared for the VOR C approach”
· “Monroeville Approach, N6E, cleared for the VOR C approach”
· “Monroeville Approach, N6E, VOR outbound”

· “Monroe County Tower, N6E, Final Approach Fix inbound, gear down and Locked”

· “Monroe County Tower, N6E, Missed Approach, field not in sight”

· “Monroeville Departure, N6E, missed approach, field not in sight, request radar vectors to the final approach course for the Monroeville VOR B approach”
· “N6E, leaving 3500 for 5000” IGP
· “Monroeville approach, N6E, turn L/R heading ​​​____, roger the weather and runway, altimeter ______” 

· “N6E, now ___ miles from MVC VOR, turn L/R heading ___, intercept the final approach course at or above 3400, cleared for the VOR B approach to Monroe county Airport, circle to land 21. Contact Monroe County Tower this freq when established inbound on the final approach course, out”
· Position, Heading, Altitude, Cleared, Freq (who, when, what) (omit pos)

· “Monroeville approach, N6E, heading, maintain altitude, cleared for the approach, contact Monroe County Tower this frequency when established inbound on the final approach course, out”

· BAC, LCL, Talk, MA

· ”Monroe County Tower, N6E, final approach course inbound, gear down and locked”
· “N6E, circle north, cleared to land RW 21”

· “Monroe County Tower, N6E, circle north, cleared to land RW 21”
· “Monroe County Tower, N6E, missed approach, runway not insight”

· “Monroeville Departure, N6E, missed approach, runway not insight, request the VOR A approach”

· “Monroeville Departure, N6E, request my alternate, Navy North Whiting, via direct, alt 8000, 2+?? Fuel remaining, 0 + 18 time enroute” IGP
