· ATIS: “Info___, 900 OVC, vis 3 miles in rain, alt 30.00, duty RW is 32”
· Complete the first 11 steps of instrument checklist

· “North Whiting Clearance Delivery, N6E, IFR to North Whiting Field, clearance on request”
· “Clearance Delivery, N6E, ready to copy”
· “N6E, is cleared to North Whiting field via the BAEYE ONE Departure to BAEYE, direct to Saufley, V-1 to Whiting, direct Whiting 305 radial 12 mile fix, maintain 8,000. Departure Freq will be 278.8, squawk______”
· “North Whiting Ground Control, N6E taxi with information___”
· “N6E, taxi to runway____”
· COMPLETE CHECKLIST, TWIST AND TOGGLE!!!

· Ensure radios, NAVIDS, transponder and CDI set for departure. VOR audio switch to on.
· “North Whiting Tower, N6E, take-off”
· “North Whiting Tower, N6E, after take-off, turn right to 340, switching to Departure, cleared for take-off”
· “Pensacola Departure, N6E, off North Whiting, passing 800 for 8,000”
· “N6E, Pensacola Departure Control, radar contact __ miles Northwest of North Whiting, report level at 8,000”

· “N6E, Wilco” IGP
· “Pensacola Departure, N6E, level 8,000”
· “N6E, contact Jacksonville Center on 251.1” 
· “N6E, contacting Jacksonville center on 251.1” IGP
· Identify PENSI using Crestview TACAN radial and DME

· “Jacksonville Center, N6E, PENSI”

· Identify BAEYE using dual navaid
· “Jacksonville Center, N6E, BAEYE”
· After Saufley, have student contact Pensacola Approach Control on 265.1

· “N6E, Contacting Approach on 265.1”

· “Pensacola Approach, N6E, level 8000, with negative information, request”

· “Roger your weather and runway, altimeter is _______, expect the TACAN 1 RWY 23 approach”

· Clear student from present position direct to BUBBA.

· “N6E, cleared direct to BUBBA”

· “N6E, hold as published at BUBBA,”

· “N6E, cleared to hold as published at BUBBA, expect further clearance at ______”
Terminal Descent: Clear for decent to 5500. 
· “N6E, you are cleared to descend to 5500”
· “Pensacola Approach, N6E, leaving 8000 for 5500”
· “Pensacola approach, N6E, holding at BUBBA, time, 5500”
· “Pensacola approach, request confirmation on EFC of ​​​​____"
· “Pensacola Approach, N6E, departing holding”
Tacan Arcing:

Lead by .8 for 150 and .6 for 120 (5% ground speed)

TACAN 1 Rwy 23 Approach (turn at 8.8 DME)

Turning inbound at 030 radial (dial 210), slow down at 015 radial, start turn at 024 radial

· “North Whiting Tower, N6E, final approach course, gear down and locked”

· “North Whiting Tower, N6E, missed approach, field not insight”

· “Pensacola Departure N6E, missed approach, field not in sight, request my alternate Bob Sikes Airport, via Direct CEW, 7000, _______ fuel remaining, 0+08 time enroute”
