DISCUSS
Precision navigation using GPS
GPS is a great tool for low level nav because it does not require line of site and at low altitudes… line of site might not be that good.
Helps even more at night because some checkpoints/features can be harder to see.

Low level navigation at night
Shall normally take place within local training area.
Contact instructor prior to brief for the route of fight.

Plan heading, time, and distance between each designated checkpoint.

Route shall be flown at 500 to 1000 AGL and between 80 and 100 KIAS.

Terminate route at either Santa Rosa OLF or one of the VFR entry points for NDZ.
PRACTICE
Night VFR navigation
Low work

Normal approach to a landing zone (LZ)

Precision approach to a landing zone (LZ)

Night power recovery autorotations

No-hover landings to a landing zone (LZ)
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