DISCUSS
GPS procedures
When being radar vectored to final remain in OBS mode.

RAIM (Receiver Autonomous Integrity Monitoring) must be available to commence the approach.  A flashing message indicator may be an indication of non-availability.

Copter GPS procedures

GPS flight plans

En route procedures

GPS approach (OBS/Leg mode, Arm/Active mode)

If aircraft is greater than 30NM from airport, CDI scale factor is at default 5NM full-scale deflection.
When within 30NM of the airport and there is an approach loaded into the flight plan the unit will transition to approach arm mode and CDI scale will smoothly change to +_ 1.0NM over the next 30 seconds and external annunciator indicates ARM

When within 2 NM from FAF and approach mode is in arm, the until will transition to approach ACTIVE mode if RAIM is available and in LEG mode. CDI scale will change smoothly to +- 0.3NM and annunciator will indicate ACTV
Mobile Regional VOR or TACAN or GPS-A

Dothan Regional VOR or TACAN or GPS-A

GPS missed approach

Automatic waypoint sequencing stops at the MAP.  If missed approach is required, manually sequence unit to the missed approach WPT.

Overlay approach

Some published approaches parallel to ground-based NAVAID-based approaches may contain transition points that do not have corresponding waypoints in the associated GPS approach.
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