DISCUSS
Failed directional gyro TACAN approach
1. Initiated by pulling HSI C/B securing power to HIS and RMI card

2. Stabilize A/C in straight and level balanced flight. Execute NATOPS procedures.

a. Shift to standby compass scan

b. If IFR, attempt to reestablish VMC

c. Troubleshoot C/Bs and turn off LAPDS

3. Troubleshoot.  Secure landing light, A/C, Pitot heats, Defog blower, Search light (LAPDS) Report problem and request radar service.

4. Level wings and look at tail of the needle to determine radial located

5. Check wet compass for magnetic heading.

6. Set appropriate course into CDI/HSI

7. Utilizing radial intercept techniques, select an intercept heading then make standard rate wet compass turns to that heading.
8. Upon intercepting the bearing, apply tracking procedures

9. Utilize full panel procedures for other maneuvers.

Lost communication while being radar vectored

If being radar vectored, by the direct route from the point of radio failure to the fix, route, or airway specified in the vector clearance

RADAR APPROACHES - initiate lost communications procedures if no transmissions are received for approximately one minute while being vectored to final, 15 seconds while on ASR final approach, or five seconds while on PAR final approach.

a.
Attempt contact on a secondary frequency, the previously assigned frequency, the tower frequency, or guard.

b.
If unable to re-establish communications and unable to maintain VMC, proceed with a published instrument approach procedure or previously coordinated instructions. Change transponder to appropriate codes.

c.
Maintain the last assigned altitude or the minimum safe/sector altitude (emergency safe altitude if more than 25 NM from the facility), whichever is higher, until established on a segment of the published approach.
INTRODUCE

Failed directional gyro TACAN Approach
Jacksonville NAS TACAN RWY 9 / Jacksonville NAS TACAN RWY 27
Mayport TACAN RWY 23 / Mayport COPTER TACAN 052

Radar vectors to TACAN final approach course (failed directional gyro)

PRACTICE

Tracking
Point to point navigation

Engine fire in flight

INDICATIONS:  FIRE light, Smoke, Flames

PROCEDURES:

WARNING

Be prepared for complete power loss.

*1. Confirm existence of fire.

If fire exists:

*2. Land immediately.

*3. Emergency shutdown - Complete After Landing.

If fire not confirmed:

*4. Land as soon as possible.

TACAN approach (full panel)

Missed approach
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