DISCUSS

Any emergency procedure
Any aircraft limitation

Course rules including Special VFR procedures

SVFR At NDZ

Min weather is 500-1

ATC shall have positive control of all SVFR traffic within Class C when field is IFR

All SVFR A/C within Class C remain at or below 700’MSL / 500’AGL, clear clouds, south of Langley Road.

SVFR to Santa Rosa go from FISH to HWY-90.  All other routing same as normal.

Use SVFR in comms.

No sim emergency within Class C when field is IFR

Searchlight/Landing light on with POS lights in steady bright within Class C.

Remain clear of C until SVFR clearance is received.
Holding is non standard (left turns) 80 knots 1 min legs at Fog, Whiskey, Echo, Igor

Holding is standard (right turns) 80 knots 1 min legs at Juniper

Number 1 A/C is approaching holding point, not necessarily first one to enter holding

Standard Operating Procedures (SOP)

Solo weather minimums for AN’s

1500-3 for both Solo ONAV and AIRNAV
Need this for your departure point, en-route, and destination for ONAV
Need this for just departure point and destination for AIRNAV
REVIEW
Checklists
Low work
Vertical takeoff/landing

Transition to forward flight

Normal approach

500’/70kias, 300’/60kias, 150’/50kias
Steep approach

500’/70kias, 300’/60kias, 300’/45kias -> 25 ° to 45 ° 
No-hover landing

Forward and down, forward and down
Stab off approach

Boost-off approach

5 foot/5 knots to the duty.

Maximum load takeoff

Check Ng at 5ft hover, do clearing turn, land, slowly pull, 40KIAS no higher than 20’
Sliding landing

Follow translational lift down (13 to 15) and touch down above translational lift (3 to 15)
Autorotation (power recovery)
Simulated engine failure at altitude

Simulated engine failure in a hover

Simulated engine failure in a taxi
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