I-2202
CD: 274.7 
Ground: 251.15
Tower: 306.925 
Dep: 278.8
· ATIS: “Info___, 1,000 OVC, vis 5 miles in light rain, altimeter 30.05, duty RW is 5”

· Complete the first 11 steps of instrument checklist

· “North Whiting Clearance Delivery, N6E___, IFR to Bob Sikes, clearance on request”

· “N6E____, roger”

· “Clearance Delivery, N6E___, ready to copy”

· “N6E___, is cleared to the Bob Sikes Airport via the Crestview One departure to Crestview. Maintain 6,000. Departure Freq will be 278.8, squawk____”

· “North Whiting Ground, N6E taxi with information___”

· “N6E, taxi to runway____”

· “N6E____, roger”

· 12-15, 16, 16

· Ensure radios, NAVIDS, transponder and CDI set for departure.

· Instrument checklist complete.

· “North Whiting Tower, N6E_____, take-off”

· “North Whiting Tower, N6E, after take-off, turn left to 010, switching to Departure, cleared for take-off”

· “Pensacola Departure Control, N6E, off North Whiting, passing ____ for 6,000”

· “N6E, Wilco” IGP
· “Pensacola Departure, N6E, level 6,000” IGP
· “N6E, approach on 272.7 when Inbound”

· **Discontinue Comms. Until radial practice is complete.

Practice:

· Tracking on 263 radial and Station Passage

· Over the Station Intercept: Intercept the ___ radial outbound (6 T’s)

· Radial Intercepts: Intercept the ___ radial outbound to inbound.

· “Crestview Approach, N6E, estimating Crestview at (2.5 miles/min), 6000 with negative info” IGP
· ATIS: Weather at Bob Sikes is 900’ OVC, 1 mile vis in light rain, altimeter ___, RW ___
· “Crestview Approach, N6E, roger runway____, altimeter ___, request VOR-B Approach”

· “Crestview Approach, N6E, cleared for the VOR-B approach, report VOR outbound”
· “Crestview Approach, N6E, VOR outboud” IGP
· BAC, LCL, Talk: “Crestview Approach, procedure turn inbound, gear down and locked”

· Analyze MAP: “Crestview Approach, N6E, VOR inbound”

· “Crestview Tower, N6E, missed approach, runway not insight”

· “Crestview Departure, N6E, request my alternate, Navy North Whiting, via Direct, alt 6000, 2+05 fuel remaining, 0+10 time enroute” IGP
· “Crestview Departure, N6E, request off freq for 1 min, will monitor guard and report back up”

· “Pensacola Approach, N6E, 6000 with North Whiting Info___”

· “Pensacola Approach, N6E, request NSE VOR RWY 14 Approach” IGP
“INSTRUMENTS CHECKED, FUEL QUANITY ___#’S LEFT, ___#’S RIGHT, WERE CURRENTLY ON THE ___ RADIAL TRACKING OUT/IN BOUND FROM _______, AT ___ DME”

