· ATIS: “Info___, 100 OVC, vis 3 miles in haze, alt 29.90, duty RW is 14”
· Complete the first 11 steps of instrument checklist

· “North Whiting Clearance Delivery, N6E, IFR to Monroe County Airport, clearance on request”
· “Clearance Delivery, N6E, ready to copy”
· “N6E, is cleared to Monroe County Airport via the DAVID ONE Departure to DAVID, direct to Monroeville, maintain 6,000. Departure Freq will be 278.8, squawk______”
· “North Whiting Ground Control, N6E taxi with information___”
· “N6E, taxi to runway____”
· COMPLETE CHECKLIST, TWIST AND TOGGLE!!!

· Ensure radios, NAVIDS, transponder and CDI set for departure. VOR audio switch to on.
· “North Whiting Tower, N6E, take-off”
· “North Whiting Tower, N6E, after take-off, turn right to 340, switching to Departure, cleared for take-off”
· “Pensacola Departure Control, N6E, off North Whiting, passing 800 for 6,000”
· “N6E, Wilco” IGP
· “Pensacola Departure, N6E, level 6,000”
· “N6E, contact Jacksonville Center on 251.1” 
· “N6E, contacting Jacksonville center on 251.1” IGP
·  “N6E, you are cleared to climb to 7000”

· “N6E, leaving 6000 for 7000”
· At 27 DME “N6E you are cleared to descend to 4500”

· “N6E leaving 7000 for 4500”

· “N6E, Contacting Approach on 351.9”

· “Monroeville Approach, N6E, level 4500, with negative information, request.”

· “Roger your weather and runway, altimeter is _______, expect the TACAN RWY 21 approach”

· Clear student from present position direct to GINNY.

· “N6E, cleared direct to GINNY”

· “N6E, hold as published at GINNY,”

· “N6E, cleared to hold as published at GINNY, expect further clearance at ______”
· “Monroeville approach, N6E, holding at GINNY, time, 4500”
· “Pensacola approach, request confirmation on EFC of ​​​​____"
· “Pensacola Approach, N6E, departing holding”
Tacan Arcing:

Lead by .8 for 150 and .6 for 120 (5% ground speed)

TACAN 1 Rwy 23 Approach (turn at 8.8 DME)

Turning inbound at 030 radial (dial 210), slow down at 015 radial, start turn at 024 radial

· “Monroe County Airport, N6E, final approach course, gear down and locked”

· “Monroe County Airport, N6E, missed approach, field not insight”

·  “Monroeville Departure N6E, missed approach, request VOR C approach.”
