· ATIS: “Info___, __________________ alt ______, duty RW is ___”
· Complete the first 11 steps of instrument checklist

· “North Whiting Clearance Delivery, N6E, IFR to Bob Sikes, clearance on request”
· “Clearance Delivery, N6E, ready to copy”
· “N6E, is cleared to the Bob Sikes Airport via the Crestview One departure to Crestview. Maintain ______. Departure Freq will be 278.8, squawk______”
· “North Whiting Ground Control, N6E taxi with information___”
· “N6E, taxi to runway____”
· “N6E, roger”
· COMPLETE INSTRUMENT CHECKLIST
· “North Whiting Tower, N6E, take-off”
· “North Whiting Tower, N6E, after take-off, turn left to 010, switching to Departure, cleared for take-off”
· Pensacola Departure Control, N6E, off North Whiting, passing 800 for ______”
· “N6E, Wilco” IGP
· “Pensacola Departure, N6E, level _______”
· “N6E, contact Crestview approach on _____ when inbound to CEW 
· “Crestview Approach, N6E, ALT with negative info” IGP 
· ATIS: Weather at Bob Sikes is___________, altimeter ___, RW ___
· “Roger Weather and Runway, altimeter _______”

VOR Holding:

· “N6E, is cleared to hold ____ of the Crestview VORTAC on the ___ radial, expect further clearance at _______”
· “Crestview Approach, N6E, holding at Crestview, _____, ALT” IGP
· “Crestview Approach, N6E, request confirmation on EFC”

· “N6E, roger, EFC time _______”
· “N6E, you are cleared to descend to ______”
· “Crestview Approach, N6E, leaving ______ for ______” IGP
· “Crestview Approach, N6E, departing holding”

Approach:
· “Crestview Approach, N6E, roger your weather and runway, altimeter _____, request VOR-B Approach”
· “Crestview Approach, N6E, cleared for the VOR-B approach, report VOR outbound” IGP
· “Bob Sikes Tower, N6E, missed approach, runway not insight”
· “Crestview Departure, N6E, missed approach, request VOR-C approach.
· “Crestview Departure, N6E, missed approach, request my alternate, Navy North Whiting, via Direct, alt 6000, 2+05 fuel remaining, 0+10 time enroute” IGP
